**SERVICE NEWS Bulletin No 14**

Re Bellett new series, Bellett 1600GTR and Florian

1966 September

Isuzu Car Company Small Car service division

**Dimensions Page**

PR91W (GTR) PR91 (GT)

Total Length 4005 4015

Height 1325 1335

Weight 970 940

Engine G161WK (DOHC) G161SS (SOHC)

**Page 9**

**(1) Overview**

The PR91W uses the PR91 base but with the G161WK DOHC engine and with a strengthened chassis. It is a fully fledged GT car with the following important points

Top Speed 190kph

0-400m 16.5 sec

Fuel Consumption 17.0km/l at 60kph

**(2) Important difference**

1.Engine

1584cc capacity, 82mmx75mm bore & stroke, 14.5/5000 kg.m/rpm torque, 120 ps/6000 rpm

2. Safety features

1) Dipping rear vision mirror for day/night vision

2) Collapsible steering column for collision safety

3) Defogger on rear screen

4) Radial tyres 165 HR-13

5) Black wiper blade and arms and anti float at speed

6) Fog lamps standard

7) Tandem master cylinder with hydro master brake booster. Rear brakes have pressure control vale to improve braking and safety

8) Limited slip differential

3. External Features

1) Front bumper split in two with fog lights in between

2) Air vents on bonnet for engine ventilation

4. Interior

1) Front seats have integrated head rest

2) Dash gauges panel and glove box lid have baked black enamel paint finish

3) Wooden gear knob

4) Clock with three hands

5. Chassis Features

1) The suspension is based on the PR91 but is heavier duty

2) Upgraded radiator

3) The petrol tank has an extra 4.6L capacity

This is followed by a detailed specification page and body schematics with measurements and then engine performance graphs, brake system, suspension details